================================================================================
                       G2DERO BIOS Release Note
================================================================================
BIOS Version:      G2DERn0.11
Project Name:      G2DERO
BIOS Core version: 5.13
Build Date:      : 2024/07/24
Author		 : LYY

[*] Files Location:

   Release Note.TXT            - This file is release document.
   AfuEfix64.efi               - BIOS Flash utility for EFI Shell X64
   Flash.nsh                   - EFI Shell batch file for update BIOS
   G2DERn006.rom               -  16MB BIOS ROM for on-line update BIOS
   MD5			       - BD7F29E63C7099671ED0734B31997838

[*] Following list is the OptionROM/FW of included in BIOS.
   AMI codebase         : 5.013_NaplesCrb_0ACIJ025
   VBIOS                : 1.02.07
   PXE OpRom            : 
   AGESA PI             : NaplesPI 1.0.0.E
   Microcode Patch      : UcodePatch_​ZP_​B1.bin 08001129,UcodePatch_​ZP_​B2.bin 0800126C
   PSP FW               : 00.07.00.83
   SMU FW               : 4.25.131.0
   ABL                  : RABLZP20050410
   APCB                 : NA
   APOB                 : NA
   APPB                 : NA

[*] Change List
Fix Bug：
1、Bug id 644-[G2DERO-B][Naples]机器不连网线去获取BMC IP地址，重启或者开关机，未提示"waitting for BMC Ready.."相关信息
Feature：

Change：
1、打开串口重定向
2、配合BMC解决WEB下打开SOL进入UEFI后，有部分显示重叠，下操作指令不会换行
3、解决在BIOS Setup下设置日期，设置无效日期也能设置保存成功
4、解决在Linux系统下执行指令dmidecode -t 3，检查机箱信息，Height 机箱高度类型显示为Unspecified
5、解决在设置IP动静态切换保存生效改变后首次在POST界面会显示BMC IP为0,BIOS Setup下BMC网络配置均显示0异常
6、解决BIOS下设置Administrator Password和User Pass，BIOS密码无法区分大小写字母
7、添加BIOS LOGO图像自适应屏幕

Flash update Note:
AfuEfix64.efi G2DERn0.11.rom /B /P /N /K /L /X /SHUTDOWN
===========================================================================
================================================================================
                       G2DERO BIOS Release Note
================================================================================
BIOS Version:      G2DERn0.10
Project Name:      G2DERO
BIOS Core version: 5.13
Build Date:      : 2024/06/19
Author		 : LYY

[*] Files Location:

   Release Note.TXT            - This file is release document.
   AfuEfix64.efi               - BIOS Flash utility for EFI Shell X64
   Flash.nsh                   - EFI Shell batch file for update BIOS
   G2DERn006.rom               -  16MB BIOS ROM for on-line update BIOS
   MD5			       - 601C13E2F9DD4F552F357D9EFA9A7F8E

[*] Following list is the OptionROM/FW of included in BIOS.
   AMI codebase         : 5.013_NaplesCrb_0ACIJ025
   VBIOS                : 1.02.07
   PXE OpRom            : 
   AGESA PI             : NaplesPI 1.0.0.E
   Microcode Patch      : UcodePatch_​ZP_​B1.bin 08001129,UcodePatch_​ZP_​B2.bin 0800126C
   PSP FW               : 00.07.00.83
   SMU FW               : 4.25.131.0
   ABL                  : RABLZP20050410
   APCB                 : NA
   APOB                 : NA
   APPB                 : NA

[*] Change List
Major change of v0.10

[2024/04/22]     
	1、屏蔽CPU压力测试GMI报错
===========================================================================

================================================================================
                       G2DERO BIOS Release Note
================================================================================
BIOS Version:      G2DERn0.06
Project Name:      G2DERO
BIOS Core version: 5.13
Build Date:      : 2023/12/26
Author		 : LYY

[*] Files Location:

   Release Note.TXT            - This file is release document.
   AfuEfix64.efi               - BIOS Flash utility for EFI Shell X64
   Flash.nsh                   - EFI Shell batch file for update BIOS
   G2DERn006.rom               -  16MB BIOS ROM for on-line update BIOS
   MD5			       - 7FA0040D107AE6BD38FCEAACDC684F02

[*] Following list is the OptionROM/FW of included in BIOS.
   AMI codebase         : 5.013_NaplesCrb_0ACIJ025
   VBIOS                : 1.02.07
   PXE OpRom            : 
   AGESA PI             : NaplesPI 1.0.0.E
   Microcode Patch      : UcodePatch_​ZP_​B1.bin 08001129,UcodePatch_​ZP_​B2.bin 0800126C
   PSP FW               : 00.07.00.83
   SMU FW               : 4.25.131.0
   ABL                  : RABLZP20050410
   APCB                 : NA
   APOB                 : NA
   APPB                 : NA

[*] Change List
Major change of v0.06

[2023/12/26]     
	1、解决pcie slot的映射问题
        2、解决BMC web下的日志报错内存位置与实际内存位置不一致
	3、解决在BIOS Setup下增加BMC用户后，在BMC web端无法使用新设置的用户登录
        4、解决点击Uesr Password之后会出现提示密码设置失败
	5、修改MCA error默认值为100
	6、解决在Bios setup设置用户密码保存重启,到Post界面输入用户密码后, Post界面左下角不显示BMC和BIOS热键信	息
	7、解决修改BIOS Setup选项Boot Feature->Option Rom Messages为Keep Current or Force BIOS时，Option 	Rom信息没有差异
        8、解决在BIOS Setup下查看BMC Firmware Revision显示不全，与BMC Web下显示有差异
	9、解决上电开机后POST界面BMC已显示了IP,依然提示"waitting for BMC Ready."等相关信息
	10、解决在BIOS Setup下打开network Stack的PXE IPv4/IPv6，在Boot选项下网卡/I350显示IPv4/IPv6时没	有"v"字
	11、修改OS下使用dmidecode -t 0查询 BIOS的版本信息
	12、开启BIOS同步BMC FRU信息功能
	13、添加 RTK USB网卡的驱动
	14、解决12盘位NV背板盘序错乱
	15、解决在0S下执行命令：dmidecode -t 39查询电源模块信息，无返回
===========================================================================
================================================================================
                       G2DERO BIOS Release Note
================================================================================
Project Name:      G2DERO
BIOS Version:      0.05
BIOS Core version: 5.13
Build Date:        08/10/2021

[*] Files Location:

   Release Note.TXT            - This file is release document.
   AfuEfix64.efi               - BIOS Flash utility for EFI Shell X64
   Flash.nsh                   - EFI Shell batch file for update BIOS
   G2SERn002.rom               - (checksum = 7f3c) 16MB BIOS ROM for on-line update BIOS

[*] Following list is the OptionROM/FW of included in BIOS.
   AMI codebase         : 5.013_NaplesCrb_0ACIJ025
   VBIOS                : 1.02.07
   PXE OpRom            : 
   AGESA PI             : NaplesPI 1.0.0.E
   Microcode Patch      : UcodePatch_​ZP_​B1.bin 08001129,UcodePatch_​ZP_​B2.bin 0800126C
   PSP FW               : 00.07.00.83
   SMU FW               : 4.25.131.0
   ABL                  : RABLZP20050410
   APCB                 : NA
   APOB                 : NA
   APPB                 : NA

[*] Change List
Major change of v0.05

[08/10/2021]     
	1. Bug 1438 - [G2DERO-B][Naples] BMC web系统清单显示PCIE slot序号与MB实际丝印不对应 
	
===========================================================================
================================================================================
                       G2DERO BIOS Release Note
================================================================================
Project Name:      G2DERO
BIOS Version:      0.04
BIOS Core version: 5.13
Build Date:        08/09/2021

[*] Files Location:

   Release Note.TXT            - This file is release document.
   AfuEfix64.efi               - BIOS Flash utility for EFI Shell X64
   Flash.nsh                   - EFI Shell batch file for update BIOS
   G2SERn002.rom               - (checksum = B6CA) 16MB BIOS ROM for on-line update BIOS

[*] Following list is the OptionROM/FW of included in BIOS.
   AMI codebase         : 5.013_NaplesCrb_0ACIJ025
   VBIOS                : 1.02.07
   PXE OpRom            : 
   AGESA PI             : NaplesPI 1.0.0.E
   Microcode Patch      : UcodePatch_​ZP_​B1.bin 08001129,UcodePatch_​ZP_​B2.bin 0800126C
   PSP FW               : 00.07.00.83
   SMU FW               : 4.25.131.0
   ABL                  : RABLZP20050410
   APCB                 : NA
   APOB                 : NA
   APPB                 : NA

[*] Change List
Major change of v0.04

[08/09/2021]     
	1. Bug 1438 - [G2DERO-B][Naples] BMC web系统清单显示PCIE slot序号与MB实际丝印不对应 
	
===========================================================================
================================================================================
                       G2DERO BIOS Release Note
================================================================================
Project Name:      G2DERO
BIOS Version:      0.03
BIOS Core version: 5.13
Build Date:        07/13/2021

[*] Files Location:

   Release Note.TXT            - This file is release document.
   AfuEfix64.efi               - BIOS Flash utility for EFI Shell X64
   Flash.nsh                   - EFI Shell batch file for update BIOS
   G2SERn002.rom               - (checksum = dfb7) 16MB BIOS ROM for on-line update BIOS

[*] Following list is the OptionROM/FW of included in BIOS.
   AMI codebase         : 5.013_NaplesCrb_0ACIJ025
   VBIOS                : 1.02.07
   PXE OpRom            : 
   AGESA PI             : NaplesPI 1.0.0.E
   Microcode Patch      : UcodePatch_​ZP_​B1.bin 08001129,UcodePatch_​ZP_​B2.bin 0800126C
   PSP FW               : 00.07.00.83
   SMU FW               : 4.25.131.0
   ABL                  : RABLZP20050410
   APCB                 : NA
   APOB                 : NA
   APPB                 : NA

[*] Change List
Major change of v0.03

[07/13/2021]
    
	1. Bug 1363 - [G2DERO-B][Naples] BIOS显示PCIE slot device不全，或与实际接入的PCI device不符
	2. Bug 1375 - [G2DERO-B][Naples] BIOS setup下设置BMC获取IP方式,保存退出后Post界面或进入BIOS setup查看，BMC网口IP显示0.0.0.0
	3. Bug 1381 - [G2DERO-B][Naples] BMC网口已做聚合，BIOS显示两个网口信息（专用和共享网口）
===========================================================================
                       G2DERO BIOS Release Note
================================================================================
Project Name:      G2DERO
BIOS Version:      0.02
BIOS Core version: 5.13
Build Date:        06/22/2021

[*] Files Location:

   Release Note.TXT            - This file is release document.
   AfuEfix64.efi               - BIOS Flash utility for EFI Shell X64
   Flash.nsh                   - EFI Shell batch file for update BIOS
   G2SERn002.rom               - (checksum = 8808) 16MB BIOS ROM for on-line update BIOS

[*] Following list is the OptionROM/FW of included in BIOS.
   AMI codebase         : 5.013_NaplesCrb_0ACIJ025
   VBIOS                : 1.02.07
   PXE OpRom            : 
   AGESA PI             : NaplesPI 1.0.0.E
   Microcode Patch      : UcodePatch_​ZP_​B1.bin 08001129,UcodePatch_​ZP_​B2.bin 0800126C
   PSP FW               : 00.07.00.83
   SMU FW               : 4.25.131.0
   ABL                  : RABLZP20050410
   APCB                 : NA
   APOB                 : NA
   APPB                 : NA

[*] Change List
Major change of v0.02

[06/22/2021]
  1.Update BMC Version (x.xx.x) in BIOS setup.
  2.Update PCIE Slot(1-10) setting in PCI Subsystem Settings.
  
===========================================================================
                       G2DERO BIOS Release Note
================================================================================
Project Name:      G2DERO
BIOS Version:      0.01
BIOS Core version: 5.13
Build Date:        06/08/2021

[*] Files Location:

   Release Note.TXT            - This file is release document.
   AfuEfix64.efi               - BIOS Flash utility for EFI Shell X64
   Flash.nsh                   - EFI Shell batch file for update BIOS
   G2SERn001.rom               - (checksum = 2315) 16MB BIOS ROM for on-line update BIOS

[*] Following list is the OptionROM/FW of included in BIOS.
   AMI codebase         : 5.013_NaplesCrb_0ACIJ025
   VBIOS                : 1.02.07
   PXE OpRom            : 
   AGESA PI             : NaplesPI 1.0.0.E
   Microcode Patch      : UcodePatch_​ZP_​B1.bin 08001129,UcodePatch_​ZP_​B2.bin 0800126C
   PSP FW               : 00.07.00.83
   SMU FW               : 4.25.131.0
   ABL                  : RABLZP20050410
   APCB                 : NA
   APOB                 : NA
   APPB                 : NA

[*] Change List
Major change of v0.01
[06/08/2021]
  1. First release for G2DERO
  


===========================================================================